PC-Dmis 2010 MR1 Object Library | Send comments on this topic. | See Object Hierarchy Chart
Feature Method
See Also

Collapse All Expand All

ID
  String value of the ID string of the feature to add as an input for a best fit or iterative alignment.

pnt_tol
  Double value of the point tolerance of the feature. Only used with best fit alignments.

# Description

Identifies Feature to be used by BF2d, BF3d, or Iterative Alignment

This function must only be called after a call to BestFit2D, BestFit3D, or Iterate

# Syntax

Visual Basic

    Public Sub Feature( _
       ByVal ID As String, _
       ByVal pnt_tol As Double _
    )

# Parameters

ID
  String value of the ID string of the feature to add as an input for a best fit or iterative alignment.
pnt_tol
  Double value of the point tolerance of the feature. Only used with best fit alignments.

# See Also

OldBasic Object

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.