### Wenzel Interface

The Wenzel interface is used with Wenzel machines with a Wenzel 2010 controller (Native Wenzel Protocol). This interface just requires a single RS232 comm port, no machine parameter file is needed from the original system.

Before starting PC-DMIS, rename the wenzel.dll to interfac.dll.

The Machine Option dialog box has two tabs for the Wenzel interface:

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).