### PC-DMIS Planner Parameters and Rules

The PC-DMIS Planner Default (IPD) file is used to define the parameters for PC-DMIS Planner within PC-DMIS. This file allows you to determine how to take hits from features within the Inspection Plan. Feature parameters are specified for Auto Features, Constructed Features, and Dimensions. You can also specify how you want to display comments and features.

The PC-DMIS Planner Rules (IPR) script is used to specify rules for how automatic processes are performed on the Inspection Plan. Rules can be modified for certain criteria. For example, the number of hits taken on a circle based upon the diameter of the circle and so forth.

Before importing an Inspection Plan from a PC-DMIS Planner CAD file or a .ip file, you need to set-up these files to apply to imported Inspection Plans.

More:

Creating and Modifying a PC-DMIS Planner Default (IPD) file

PC-DMIS Planner Rules (IPR) script