### Manmiti Interface

The Manmiti interface is used with Mitutoyo Manual machines with MAG-1, MAG-2, or MAG-3 controllers that connect to the scales. This is a GPIB interface.

Before starting PC-DMIS, rename the manmiti.dll to interfac.dll.

The Machine Option dialog box has two tabs for the Manmiti interface:

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).