### Material Conditions

The Material Conditions area contains the following tolerancing methods:

Option button | Stands For | Description
M | MMC | Maximum material condition applied to either the feature or a datum.
R | RFS | Regardless of feature size applied to either the feature or a datum.
L | LMC | Least material condition applied to either the feature or a datum.

Currently you can select Material Condition modifiers for True Position, Parallelism, and Perpendicularity dimensions.

Be aware that for True Position dimensions, selecting the Use Datums check box will cause the XYZ output values to use the alignment of the datums.

More:

Recall Button