#### Constraints for 3D Best Fit Alignments

There are also constraints that can be applied to 3D Best Fit alignments. The constraint options are:

1. Rotate and Translate (default) – This allows the alignment full flexibility while correlating the machine data to the theoretical values.

2. Rotate Only – This option restricts the alignment to rotation only, without applying any translations.

3. Translate Only – This option restricts the alignment to translation only, without applying any rotations.