Current Help System: PC-DMIS CMM (View Core Help)

#### Move Speed

The Move Speed box allows you to specify the move speed for the PH9 calibration.

To change the Move Speed value:

1. Select the Move Speed box.

2. Type a new move speed value. This value should be a percent between 1% and 100%, with 1.0 being the slowest and 100.0 the fastest.

See "Move Speed %" in the "Setting your Preferences" section of the PC-DMIS Core documentation for additional ways to affect the speed in the measurement process.

Note: The number in the Move Speed box can contain no more than four decimal places. If a number with more than four decimal places is entered, PC-DMIS rounds the number off at the fourth decimal place.