Current Help System: PC-DMIS Fixturing (View Core Help)

### To Verify a Fixture Definition

This procedure determines whether or not a column can be set at the selected fixture point. This checks the location of that point, making sure a column placed there fits within the defined machine volume and that no collisions occur with the part or with other fixtures.

1. Select the
   Insert | Hardware Definition | Fixture menu option to access the Create/Modify Fixture dialog box.

2. Select the Fixture Points tab.

3. Select the fixture from the Available Fixtures list.

4. Select a fixture point from the list.

5. Click the Verify button. PC-DMIS displays a message box stating the result of the verification.