Current Help System: PC-DMIS Laser (View Core Help)

### COP Command Mode Text

The COP command inside the Edit window’s Command Mode looks like this:

COP1 =COP/DATA,SIZE=0
REF,,

The COP command must precede any scan referring to it in the part program.

For example REF,SCN2 below points to the SCN2 scan and will use its data:

COP2 =COP/DATA,SIZE=0
REF,SCN2,,

You can have more than one scan refer to a COP command.