Current Help System: PC-DMIS Laser (View Core Help)

#### Perceptron Sensor

Laser Sensor tab pointing to the binary file for Perceptron Sensor

Use the … button to browse to the location of the CSGMain.bin binary file in the Sensor Binary File box. This file has the sensor configuration that came with your probe and is installed when you install the toolkit and drivers for the probe.

Specifying the Hardware from the drop-down list allows PC-DMIS to remember what the options (Greysums, V5 Projectors, Flat Target Calibration, etc.) should be allowed/disallowed even when you are offline. When offline, all the options for the selected hardware type are available for revision.

Clicking AutoDetect will check the hardware that is currently attached to your machine. This will verify the hardware specified in the Hardware drop-down list is correct..