Current Help System: PC-DMIS Portable (View Core Help)

### Aiming tab

Machine Options dialog box - Aiming tab

Motors On: Engages the horizontal and vertical tracker head motors in order to allow manual tracker head movement.

Motors Off: Releases the horizontal and vertical tracker head motors in order to allow manual tracker head movement.

Tracker Pad:

Control buttons (Left, Up, Right, Down): Clicking the control buttons will move the laser in the respective direction. Click a control button once and the tracker slowly begins to move until you click Stop. Each successive click will cause the tracker to move more quickly in that direction. The black box in the middle of these buttons will flash with a green indicator when the reflector is considered to be settled.

Move Distance: This value provides the approximate distance at which the laser will search for the reflector when you click Search. Moving the associated slider to the right will increase the Move Distance value will moving it to the left will decrease the value.

Search Diameter: Provides the diameter for the search area at the approximate Move Distance when you click Search. Moving the associated slider to the right will increase the Search Diameter value will moving it to the left will decrease the value.

Take Hit: Will measure a stationary hit (same as Ctrl-h) at the current location of the reflector.