Current Help System: PC-DMIS Settings Editor (View Core Help)

### Iter Align Point Tol Default

This vector point tolerance value in the Edit window (as PNT TOL = n) to specify the vector point tolerance for manual touches in an iterative alignment.

Entry Name: IterAlignPointTolDefault

Entry Type: Real Number specifying tolerance distance. Default value is 5.

User permission is required to change entry