Current Help System: PC-DMIS Settings Editor (View Core Help)

### External Rotab Move Timeout

Specifies a timeout for response to a requested table move. A value of 0.0 disables this timeout. If the timeout occurs, the user will be prompted as to whether or not to try resending the command for which the response was not received within the allowed time.

Entry Name: ExternalRotabMoveTimeout

Entry Type: Real Number specifying seconds. Default value is 0 (no timeout).

User permission is required to change entry