Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision ParCalibration Retries

If a measurement during ParFocal or ParCentral Calibration fails, the calibration will retry up to the number of times as indicated by this value.

Entry Name: ProbeQualVisionParCalibrationRetries

Entry Type: Whole Number to specify number of retries. Default value is 3.

User permission is required to change entry