Current Help System: PC-DMIS Settings Editor (View Core Help)

### Multi Sec Scan Incr

Specifies the distance between sections for a Multisection Manual scan if you will be scanning across multiple sections. For parallel planes and circles, this is a distance, for radial planes this value is an angle. PC-DMIS automatically spaces the sections on the part.

Entry Name: MultiSecScanIncr

Entry Type: Real Number specifying distance or angle. Default value is 0.1.

User permission is required to change entry