Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Shank Offset

Determines the distance (or length) up from the tip of the shank that PC-DMIS will take the next set of qualification hits. This value is only used when the "ProbeShankCheck" option is set to TRUE (1).

Entry Name: ProbeShankOffset

Entry Type: Whole Number specifying distance. Default value is 5.

User permission is required to change entry