Current Help System: PC-DMIS Settings Editor (View Core Help)

### Penalty PH10

Provides an approximate time in seconds taken by a CMM to change a PH10 probe tip. This penalty specifies that all features measured with the PH10 probe tip will be grouped together and sorted within the PH10 probe tip group.

Entry Name: Penalty_PH10

Entry Type: Real Number to specify seconds. Default value is 3.

User permission is required to change entry