Current Help System: PC-DMIS Settings Editor (View Core Help)

### Circle CG Gray Sum Max

Provides the maximum pixel intensity beyond which pixels exceeding this value will not be used. This value is used when measuring laser circle features using the Gray Sum locater type.

Entry Name: Circle_CGGraySumMax

Entry Type: Whole Number specifying maximum pixel intensity. Default value is 200.

User permission is required to change entry