Current Help System: PC-DMIS Settings Editor (View Core Help)

### Command Identification - ID Starting Number

The Starting Number value determines the first number that will be used in the identification process. Any number between 1 and 9999 can be entered.

Entry Name: (A,C,COPOper,CS,D,FCF,F,L,Q,V)Start(0-17)

Entry Type: Whole Number to specify starting number. Default value is 1.

User permission is required to change entry

Note: Preferably this value should be set from the ID Setup tab of the SetUp Options (F5) dialog box within PC-DMIS.

Command Key:

AStart0 | Alignments
CStart0 | Comments
COPOperStart0 | Pointcloud Operator
CSStart0 | Call Subs
DStart(0-16) | Dimension/Angle - Symmetry
FCFStart(0-16) | Feature Control Frame
FStart(0-17) | Feature/Blobs - Surfaces
LStart0 | Label
QStart0 | SPC Queries
VStart0 | Variables

See Also:

Command Identification - ID Length

Command Identification - ID Letters