Current Help System: PC-DMIS Settings Editor (View Core Help)

### ACR2 Measured Origin

Provides the XYZ offset in mm that is used during calibration of an ACR2 probe change rack. It establishes the origin for an ACR2 port after measuring the location of the pin inside the port. You should not normally need to modify this setting.

Entry Name: ACR2_MeasuredOrigin

Entry Type: Character String specifying tool changer origin. Default value “Default value “113.55 14.5 -31.5”.

User permission is required to change entry