Current Help System: PC-DMIS Settings Editor (View Core Help)

### Distance To CAD Edge Tolerance

Provides the tolerance value within which PC-DMIS will search from a feature's centroid to the nearest CAD edge. This is used in determining the label type that should be used.

Entry Name: DistanceToCADEdgeTolerance

Entry Type: Real Number specifying distance in MM. Default value is 10.

User permission is required to change entry