Current Help System: PC-DMIS Settings Editor (View Core Help)

### Keep DCI IP File

When importing an IP file contained within the CAD file, this option controls if an external copy of the IP file is saved. Setting this value to TRUE, will save an external copy of the imported IP file. This allows you to inspect the .ip text file to see the exact IP commands that were generated.

Only the AIMS, CATIA 5, and UG DCIs use this value.

Entry Name: KeepDCIIPFile

Entry Type: True/False value. Default value is FALSE.

User permission is required to change entry