Current Help System: PC-DMIS Settings Editor (View Core Help)

### Min Time Delta Between Points In Milliseconds

Allows PC-DMIS to reduce the amount of points that are scanned by deleting hits that are read in faster than the specified time delay.

Entry Name: MinTimeDeltaBetweenPointsInMilliseconds

Entry Type: Whole Number to specify time in Msec. Default value is 0.

User permission is required to change entry