Current Help System: PC-DMIS Settings Editor (View Core Help)

### Pass Back Settings From Subroutine

This option allows changes made by a subroutine update to the current alignment to be seen by the main program after the subroutine call. This would also apply to any other system changes that occur in the subroutine. When this value is set to TRUE (1), settings could be passed from the subroutine.

Entry Name: PassBackSettingsFromSubroutine

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry