Current Help System: PC-DMIS Settings Editor (View Core Help)

### Upper Bound

Provides the maximum distance (in pixels) that included points can be from each other along scanlines. The range of values is between 1 and 100. The minimum value of 1 will retain each and every column (i.e. 100% sampling). The maximum value of 100 will retain 16 points per full line with a V5 or 8 points per line with a V4i. This referred to as "Regular Spacing" for Column Sampling Rate density type.

Entry Name: UpperBound

Entry Type: Whole Number specifying distance in pixels. Default value is 100.

User permission is required to change entry