Current Help System: PC-DMIS Settings Editor (View Core Help)

### Target Edge Selection Type

This value determines the Target Edge Selection method that will be used to detect a Target Edge. See the "Automatic Hit Target - Edge Parameter Set" topic in the PC-DMIS Vision help file for more information.

Entry Name: TargetEdgeSelectionType

Entry Type: Whole Number specifying selection type. Default value is 2.

User permission is required to change entry

Target Edge Selection Type Key:

0 | Dominant Edge
1 | Nearest Nominal
2 | Matching Edge
3 | Specified Edge