Current Help System: PC-DMIS Settings Editor (View Core Help)

### Patch Closed

This option determines if the feature created with Patch Scan is closed (cylinder, cone, slot etc.). With this option set to TRUE (1), PC-DMIS reduces the number of boundary points needed to define the scan boundary. You would only need to enter the Start and Direction points and an End point.

Entry Name: PatchClosed

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.

User permission is required to change entry