Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Edge Scan Length

This value is used for the vision probe tip offset calibration. The length value is expressed as a fraction of the smaller axis dimension of the live image size and thus would be less than 1.

Entry Name: ProbeQualVisionEdgeScanLength

Entry Type: Real Number specifying length. The default is 0.15.

User permission is required to change entry