Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision ParCalibration Percent Detection

Provides a percentage of detected points versus anticipated points that are used in determining success or failure during ParCentral Calibration. For Example, If you set this value to 50 and you are measuring a circle target over the circle standard. The Calibration anticipates a measure of 200 points but only measures less than 100 points because the circle target is not well placed over the circle target. This measurement would count as a failure.

Entry Name: ProbeQualVisionParCalibrationFocusSamples

Entry Type: Whole Number to specify percentage of points. Default value is 60.

User permission is required to change entry