Current Help System: PC-DMIS Settings Editor (View Core Help)

### Vision DCC FOV Split WH Percent

When a rectangular region is used to determine if an ROI fits in the FOV then this setting defines the percentage of the FOV to use. This used in DCC mode or when the "VisionDCCFOVSplitSafeMode" value is set to FALSE.

Entry Name: VisionFOVSplitWHPercent

Entry Type: Whole Number to specify percent. Default value is 95.

User permission is required to change entry