Current Help System: PC-DMIS Settings Editor (View Core Help)

### Scan Animate Every N Pts Collision Detection

Scanning animation for offline programming allows you to limit the number of points that are used for the animation. For example, If you set this value to 10, PC-DMIS will only take every 10th point, plus the first and last points. This accommodates collision detection as well. This value is used for probe movement during collision detection.

Entry Name: ScanAnimateEveryNPtsCollisionDetection

Entry Type: Whole Number to specify the number of scan points. Default value is None (1).

User permission is required to change entry