Current Help System: PC-DMIS Settings Editor (View Core Help)

### Disable 2 Sided Lighting

When this value is set to TRUE, two-sided lighting is disabled and back face culling is used during rotation. The resulting lighting effects will roughly display only half of the CAD elements.

Entry Name: Disable2SidedLighting

Entry Type: True/False value. Default value is FALSE.

User permission is required to change entry