Current Help System: PC-DMIS Settings Editor (View Core Help)

### Auto Features - Permanent Hits

Specifies the default Permanent Hits value that will be used in the creation of Auto Features. Permanent Hits are used to measure the plane around the nominal point location for the specified feature. Permanent sample hits are taken for all subsequent measurements during execution of the part program after the initial measurement. See the "Auto Features – Initial Hits" topic.

Entry Name: DCC(Angle,Edge,Surf)PermHits

Entry Type: Whole Number to specify the number of Permanent hits. Default value is 3.

User permission is required to change entry