Current Help System: PC-DMIS Settings Editor (View Core Help)

### RMS Tolerance In MM

Provides the tolerance in millimeters, beyond which the RMS value is considered to be out-of-tolerance. The action specified by the "RMSOutTolAction" will be executed when the RMS value is out-of-tolerance.

Entry Name: RMSToleranceInMM

Entry Type: Real Number to specify tolerance in MM. Default value is 0.1.

User permission is required to change entry