Current Help System: PC-DMIS Settings Editor (View Core Help)

### DMIS Max Measurement Velocity MMPS

This value should be set to the maximum measure speed of your machine in millimeters per second. This value is translated for the Top Speed value on the Part/Machine tab of the Setup Options dialog box. When these two values are set correctly, then commands will be translated correctly. For example, if you have set this value to 16.6 and the Top Speed value to 383mm/sec, then TOUCHSPEED commands will be correct.

The "DMISFedratPcntOfMaxMachineSpeed" should be set 0 when this value is set.

Entry Name: DMISMaxMeasurementVelocityMMPS

Entry Type: Real Number specifying millimeters per second. Default value is -1.

User permission is required to change entry