Current Help System: PC-DMIS Settings Editor (View Core Help)

### Point Tolerance Minus

Provides the negative tolerance from the nominal, and is specified in current part program units. Points that are less than this value from the nominal will be colored based on the standard PC-DMIS plus tolerance color.

Entry Name: PointToleranceMinus

Entry Type: Character String to specify distance. Default value is None ( ).

User permission is required to change entry