Current Help System: Tutor Translator (View Core Help)

### Plane Measurement Commands

MPL (MEMORY [10], 3)
MPL (MEMORY [10], 3, FORM LSM) translates to è

ASSIGN/E.BADMEAS=0

PLN3 = FEAT/PLANE, RECT

THEO/<1,0,-9.9995>,<0,0,1>
ACTL/<1,0,-9.9995>,<0,0,1>
MEAS/PLANE, 3
…
… move/hit/tip commands
…
ENDMEAS/

ASSIGN/E.WM2=E.WM1
ASSIGN/E.WM1 = TUTORELEMENT(”PLN3")
ASSIGN/E.MEMORY [10] = E.WM1
…
… Evaluation commands.
…

The following command that uses ISO algorithm does not have an equivalent PC-DMIS command. See the section on ”Measurement Commands with no PC-DMIS Equivalent” for more information.

MPL (MEMORY [10], 3, FORM ISO)