Current Help System: Tutor Translator (View Core Help)

### Measurement Commands with no PC-DMIS Equivalent

Some Tutor commands have no equivalent PC-DMIS commands and are approximately translated. For example, fixed axis cones are translated as generic cones and A Paraboloid or a Torus is translated as a measured Points Set. A Comment/Oper command has been added in order to notify the operator about missing compatibility with the original Part Program. A Comment/Oper command has been added for ISO commands as well.

ISO Commands

Measurement commands that use the ISO algorithm don’t have an equivalent PC-DMIS command. The commands are approximately translated similar to a command that uses a Least Square algorithm.

The Measurement Command examples given below do not represent all of the possible measurement commands, but do provide a representative list of examples. All Tutor commands are listed, but not all their possible parameter combinations are given.