Current Help System: Tutor Translator (View Core Help)

#### Not Aligned Circle

PC-DMIS does not have a corresponding measured feature for a not aligned circle. This command is translated as two different PC-DMIS commands.

MCIR_NA(MEMORY[2],7) translates to è

ASSIGN/E.BADMEAS=0

PLN2 =FEAT/PLANE,RECT

THEO/<1.8618,-1.1968,1.8671>,<-0.7975331,-0.6032664,-0.0032448>,1,0
ACTL/<1.8618,-1.1968,1.8671>,<-0.7975331,-0.6032664,-0.0032448>,1,0
MEAS/PLANE,3
…
… move/hit/tip commands. The number of hits is always 3.
…
ENDMEAS/

CIR7 =FEAT/CIRCLE,RECT,OUT,LEAST_SQR

THEO/<2.0037,3.0008,0.12>,<-0.7975331,-0.6032664,-0.0032448>,12.663,0
ACTL/<2.0037,3.0008,0.12>,<-0.7975331,-0.6032664,-0.0032448>,12.663,0
MEAS/CIRCLE,4,FEATURE=PLN2
…
… move/hit/tip commands. The number of hits is the number defined in the MCIR_NA command minus the 3 hits of the plane.
…
ENDMEAS/

ASSIGN/E.WM2=E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("CIR7")
ASSIGN/E.MEMORY[2]= E.WM1
…
… Evaluation commands.
…