Current Help System: Tutor Translator (View Core Help)

### Middle Point Construction Commands

The command is translated in the corresponding PD-DMIS command

IMIDPT (MEMORY[40], 2, MEMORY[101]) translates to è

PNT58 = FEAT/POINT,RECT

THEO/<152.0015,177.001,135.0005>,<0.0099995,0,0.99995>
ACTL/<152.0015,177.001,135.0015>,<0.0099995,0,0.99995>
CONSTR/POINT,MID,E.MEMORY[101].ID,E.MEMORY[102].ID

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("PNT58")
ASSIGN/E.MEMORY[40] = E.WM1
…
… Evaluation commands.
…

IMIDPT (MEMORY [41], MEMORY[103],MEMORY[106]) translates to è

PNT60 =FEAT/POINT,RECT

THEO/<152.0035,177.001,119.002>,<0.0099995,0,0.99995>
ACTL/<152.0035,177.001,119.002>,<0.0099995,0,0.99995>
CONSTR/POINT,MID,E.MEMORY[103].ID,E.MEMORY[106].ID

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("PNT60")
ASSIGN/E.MEMORY[41] = E.WM1
…
… Evaluation commands.
…