Current Help System: Tutor Translator (View Core Help)

### THEO Commands

The THEO command is translated as an assignment of a TH table field.

THEO (X=10.0,UX=0.002,LX=0.002) translates to è

ASSIGN/E.TH.X.N = 10.0
ASSIGN/E.TH.X.UT = 0.002
ASSIGN/E.TH.X.LT = 0.002

The OOT_COND and NO_OOT_COND commands do not have effect

Tutor allows the assignment of DMS decimal format values to angle fields (A,AXY,AYZ and AZY). PC-DMIS only allows the assignment of decimal format values to angle fields. Therefore, the values is converted using the DMS2DEG function:

THEO (A=10.4534,UA=0.0015,LA=0.0015) translates to è

ASSIGN/TH.A.N = DMS2DEG(10.4534,OFMT.DMS)
ASSIGN/TH.A.UT = DMS2DEG(0.0015,OFMT.DMS)
ASSIGN/TH.A.LT = DMS2DEG(0.0015,OFMT.DMS)

NONCRITICITY(X=40,Y=50,Z=40) translates to è

ASSIGN/TH.X.NC = 40.0
ASSIGN/TH.Y.NC = 50.0
ASSIGN/TH.Z.NC = 40.0

The NONCRITICITY command does not have effect