Current Help System: Tutor Translator (View Core Help)

#### Symmetry

Tutor allows the following symmetry commands:

- Checked Line – Datum Line.

- Checked Line – Datum Plane.

- Checked Plane – Datum Line.

- Checked Plane – Datum Plane.

- Checked Line – Datum Middle Line.

- Checked Line – Datum Middle Plane.

- Checked Plane – Datum Middle Line.

- Checked Plane – Datum Middle Plane.

where:

- Line means Class Line feature: Line, Cylinder and Cone.

GEO_TOL(SYMM,MEMORY[122], MEMORY[123]) translates to è

DIM SYM1= SYMMETRY OF CONE E.MEMORY[122].ID TO CYLINDER E.MEMORY[123].ID UNITS=IN ,$ GRAPH=OFF TEXT=OFF MULT=10.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 0.0000 0.0000 0.0000 0.0000 0.0000 #--------

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.MEMORY[122].TP = SYM1.MEAS
ASSIGN/E.MEMORY[122].GTOL = 7
ASSIGN/E.WM1 = E.MEMORY[122]

GEO_TOL(>MEMORY[200],SYMM,MEMORY[122], MEMORY[123]) translates to è

DIM SYM1= SYMMETRY OF CONE E.MEMORY[122].ID TO CYLINDER E.MEMORY[123].ID UNITS=IN ,$ GRAPH=OFF TEXT=OFF MULT=10.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 0.0000 0.0000 0.0000 0.0000 0.0000 #--------

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = E.MEMORY[122]
ASSIGN/E.WM1.TP = SYM1.MEAS
ASSIGN/E.WM1.GTOL = 7
ASSIGN/E.MEMORY[200] = E.WM1

GEO_TOL(SYMM,MEMORY[122],MIDDLE, MEMORY[123], MEMORY[124]) translates to è

SYM1_LIN1 =FEAT/LINE,RECT,UNBND

THEO/<68,13,14>,<0.8880738,0.3250576,0.3250576>
ACTL/<68,13,14>,<0.8880738,0.3250576,0.3250576>
CONSTR/LINE,MID,E.MEMORY[123].ID,E.MEMORY[124].ID,112
DIM SYM1= SYMMETRY OF CONE E.MEMORY[122].ID TO LINE SYM1_LIN1 UNITS=IN ,$ GRAPH=OFF TEXT=OFF MULT=10.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 0.0000 0.0000 0.0000 0.0000 0.0000 #--------

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.MEMORY[122].TP = SYM1.MEAS
ASSIGN/E.MEMORY[122].GTOL = 7
ASSIGN/E.WM1 = E.MEMORY[122]

GEO_TOL(>MEMORY[200],SYMM,MEMORY[122],MIDDLE, MEMORY[123], MEMORY[124]) translates to è

SYM1_LIN1 =FEAT/LINE,RECT,UNBND

THEO/<68,13,14>,<0.8880738,0.3250576,0.3250576>
ACTL/<68,13,14>,<0.8880738,0.3250576,0.3250576>
CONSTR/LINE,MID,E.MEMORY[123].ID,E.MEMORY[124].ID,112
DIM SYM1= SYMMETRY OF CONE E.MEMORY[122].ID TO LINE SYM1_LIN1 UNITS=IN ,$ GRAPH=OFF TEXT=OFF MULT=10.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 0.0000 0.0000 0.0000 0.0000 0.0000 #--------

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = E.MEMORY[122]
ASSIGN/E.WM1.TP = SYM1.MEAS
ASSIGN/E.WM1.GTOL = 7
ASSIGN/E.MEMORY[200] = E.WM1