Current Help System: Tutor Translator (View Core Help)

#### Angularity

ANGOL(MEMORY[120], MEMORY[123]) ) translates to è

DIM ANGLRTY1 =ANGULARITY FROM LINE E.MEMORY[120].ID TO CYLINDER E.MEMORY[123].ID EXTENDLENGTH=0.0000 ANG=0.1000 UNITS=IN ,$
GRAPH=OFF TEXT=OFF MULT=0.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 9.9825 4.9913 4.9913 9.9825 9.9725 ------>

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.MEMORY[120].TP = ANGLRTY1.MEAS
ASSIGN/E.MEMORY[120].GTOL = 4
ASSIGN/E.WM1 = E.MEMORY[120]

ANGOL(>MEMORY[130], MEMORY[120], MEMORY[123],0.1) translates to è

DIM ANGLRTY2 =ANGULARITY FROM LINE E.MEMORY[120].ID TO CYLINDER E.MEMORY[123].ID EXTENDLENGTH=0.0000 ANG=0.1000 UNITS=IN ,$
GRAPH=OFF TEXT=OFF MULT=0.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 9.9825 4.9913 4.9913 9.9825 9.9725 ------>

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = E.MEMORY[120]
ASSIGN/E.WM1.TP = ANGLRTY2.MEAS
ASSIGN/E.WM1.GTOL = 4
ASSIGN/E.MEMORY[130] = E.WM1

ANGOL DIST(MEMORY[120], MEMORY[123],0.1,6.) translates to è

DIM ANGLRTY3 =ANGULARITY FROM LINE E.MEMORY[120].ID TO CYLINDER E.MEMORY[123].ID EXTENDLENGTH=12.0000 ANG=0.1000 UNITS=IN ,$
GRAPH=OFF TEXT=OFF MULT=0.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 8.4705 4.2352 4.2352 8.4705 8.4605 ------>

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.MEMORY[120].TP = ANGLRTY3.MEAS
ASSIGN/E.MEMORY[120].GTOL = 4
ASSIGN/E.WM1 = E.MEMORY[120]]

ANGOL DIST(MEMORY[120], MEMORY[123],0.1, DISTVAR) translates to è

Where the variable DISTVAR contains the dist value.

DIM ANGLRTY5 =ANGULARITY FROM LINE E.MEMORY[120].ID TO CYLINDER E.MEMORY[123].ID EXTENDLENGTH=DISTVAR*2 ANG=0.1000 UNITS=IN ,$
GRAPH=OFF TEXT=OFF MULT=0.00 OUTPUT=NONE

AX NOMINAL +TOL -TOL MEAS MAX MIN DEV OUTTOL
M 0.0000 0.0100 0.0000 8.4705 4.2352 4.2352 8.4705 8.4605 ------>

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.MEMORY[120].TP = ANGLRTY5.MEAS
ASSIGN/E.MEMORY[120].GTOL = 4
ASSIGN/E.WM1 = E.MEMORY[120]

Warning: For commands where the checked element is a plane, the datum element is a line and the DIST is required the following comment is written in place of the tolerance:

COMMENT/DOC,=====================================
,WARNING: ANGULARITY BETWEEN PLANE AND
,LINE USING PROJECTION, DISTANCE IS NOT ALLOWED
,==================================================