Current Help System: Tutor Translator (View Core Help)

### Measurement Commands that May Have a PC-DMIS Equivalent

Measurement Commands that may or may not have equivalent commands in PC-DMIS but do have construction commands are translated:

- If RefSysNum is defined the associated reference system is recalled:
  RECALL/ALIGNMENT,INTERNAL, E.ALIGNMENTS[RefSysNum]

- If RefSysNum is defined the current reference system is recalled:
  RECALL/ALIGNMENT,INTERNAL, E.ALIGNMENTS[E.CUR_ALIGN]

- Copy Structure - Copy the structure of E.WM1 from E.WM2.
  ASSIGN/E.WM2 = E.WM1

- Data Memorization in the structure E.WM1.

- If the memory of destination is not E.WM1, data is stored also in the destination memory structure.

- Dimension Command and True Position computing if necessary

- Profile Command - Computing if necessary

- Evaluation output. - For more information, see Element Evaluation.