Current Help System: Tutor Translator (View Core Help)

### Sphere Measurement Commands

The following commands that use ISO algorithm don’t have an equivalent PC-DMIS command. See the section on ”Measurement Commands with no PC-DMIS Equivalent” for more information.

MSPH (MEMORY [10], 6)
MSPH (MEMORY [10], 6, FORM ISO) translates to è

ASSIGN/E.BADMEAS=0

SPH1 = FEAT/SPHERE,RECT,IN

THEO/<10,20,30>,<0,0,1>,23
ACTL/<10,20,30>,<0,0,1>,23
MEAS/SPHERE,5
…
… move/hit/tip commands
…
ENDMEAS/

ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMENT("SPH1")
ASSIGN/E.MEMORY[10] = E.WM1
…
… Evaluation commands.
…