Current Help System: PC-DMIS Vision (View Core Help)

#### A Note on Optical Tips

The concept of a Vision probe parallels a contact probe to a certain point. Obviously a Vision probe doesn't come in physical contact with the part, but both contact probes and optical probes use the term "probe tip
" to specify various positions of an articulating probe head. The actual tip on a Vision probe contains the optical device (the camera).

If you select a probe from the Probes list or a probe tip from the Probe Tips list, PC-DMIS Vision inserts a LOADPROBE/ command or a TIP/ command respectively into the Edit window.

When PC-DMIS Vision executes these commands, it performs its associated probe definition.