Current Help System: PC-DMIS Vision (View Core Help)

### How AutoTune Execution Works

When you execute your part program in AutoTune execution, PC-DMIS Vision steps you through the program, feature by feature.

It performs a test measurement on each feature and then displays the Auto Features dialog box for that feature.

You then have the option to apply one or more of those changes to one or more subsequent features in the part program.

Once you are satisfied with the feature and click OK, PC-DMIS Vision then tests the next feature. It continues doing this until the entire part program has been executed in AutoTune execution

Once you finish executing the part program in AutoTune execution, you can return to regular Execute mode.