PC-Dmis 2010 MR2 Object Library | Send comments on this topic. | See Object Hierarchy Chart
CopyMeasToNom Property
See Also

Collapse All Expand All

# Description

Read/Write: Flag that causes measured values to be copied to nominal values after execution

Property used to indicate/set whether the object should execute in MASTER mode. After executing in MASTER mode, the object copies the measured vector, centroid, and other nominal information to the nominals and turns off MASTER mode. This copies the same information that gets calculated using the CalculateNominals method.

# Property type

Read-write property

# Syntax

Visual Basic

    Public Property CopyMeasToNom() As Boolean

# Return Type

Read/write Boolean.

# Remarks

The nominal information that this copies includes the following:

- CENTROID
- VECTOR
- DIAMETER
- STARTPOINT
- ENDPOINT
- BALLCENTER
- LENGTH
- ELLIPSEMINORAXIS
- ANGLE
- SURFACEVECTOR
- THICKNESS
- NUMHITS
- SPACER
- INDENT
- AUTO_MOVE_DISTANCE
- DEPTH
- TARG
- SCANROWCOUNT
- ANGLE_VECTOR
- PUNCH_VECTOR
- PIN_VECTOR
- PIN_DIAMETER
- REPORT_VECTOR
- REPORT_SURF_VECTOR
- HEIGHT
- MEASURE_VECTOR
- UPDATE_VECTOR
- CORNER_RADIUS
- ANGLE2

# See Also

Command Object

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.