PC-Dmis 2010 MR2 Object Library | Send comments on this topic. | See Object Hierarchy Chart
AddBoundaryPoint Method
See Also

Collapse All Expand All

X
  Double value representing the X value of the boundary point.

Y
  Double value representing the Y value of the boundary point.

Z
  Double value representing the Z value of the boundary point.

# Description

Adds a boundary point to a scan This function is used to add the initial point, end point, and other boundary points in the case of patch scans. It should be called for each boundary point to be added. It should not be called more than num_bnd_pnts times (as specified in the call to StartScan).

# Syntax

Visual Basic

    Public Sub AddBoundaryPoint( _
       ByVal X As Double, _
       ByVal Y As Double, _
       ByVal Z As Double _
    )

# Parameters

X
  Double value representing the X value of the boundary point.
Y
  Double value representing the Y value of the boundary point.
Z
  Double value representing the Z value of the boundary point.

# See Also

OldBasic Object

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.