PC-Dmis 2010 MR2 Object Library | Send comments on this topic. | See Object Hierarchy Chart
Type Property
See Also

Collapse All Expand All

# Description

Read/Write: Type of scan control point This specifies the type of control point.

# Property type

Read-write property

# Syntax

Visual Basic

    Public Property Type() As BSCTRLPT_ENUM

# Return Type

Read/write BSCTRLPT_ENUM.

# Remarks

There are four types of control points:

1. Plane (uses these elements: Plane, X,Y,Z,I,J,K,Num Crossings, Scan Speed, Point Density)
2. Sphere (uses these elements: Sphere, X, Y, Z, I, J, K, Num Crossings, Scan Speed, Point Density, Diameter)
3. Cone (uses these elements: Cone, X, Y, Z, I, J, K, Num Crossings, Scan Speed, Point Density, Angle)
4. Cylinder (uses these elements: Cylinder, X, Y, Z, I, J, K, Num Crossings, Scan Speed, Point Density, Diameter)

# See Also

ControlPoint Object

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.